**1’S AND 2’S COMPLEMENT OF 8 BIT NUMBER:**

LDA 3000

CMA

STA 3001

ADI 01

STA 3002

HLT

